THREE WIRE BIVY SET UP INSTRUCTIONS:

1. Remove contents from stuff sack. Spread bivy body out on ground.

2. Assemble the two poles. Be careful to insert each pole section into the next by hand instead of allowing the shock cord to snap them together to ensure each pole section is fully seated.

3. Thread the long pole through the sleeve and insert the pole tips into grommets on each side of the head of the bivy.

4. Insert the shorter pole with blunt ends into the black webbing pockets located at the top of the bivy hood.

5. Attach all “Twist Clips” to the pole.

6. Stake out the three webbing loops at the head and two loops at the foot of the bivy.

Separate 6”, large diameter pole segment included for emergency field repair. Slide repair pole over the break to act as a splint.

HELPFUL HINTS FOR TENT SET UP

Unzip the opening of the bivy when folding or stuffing to allow air to escape.
Our tents are easy to set up, but we suggest you practice once at home before using them for the first time to avoid late night bickering with tent mates while fumbling around in the dark.
Before pitching tent, clear campsite of debris that may pierce tent floor.
We recommend staking out all corners, vestibules and guylines to increase space and ventilation. Securely staking out your tent and all guylines is crucial to maintaining the structural integrity of your tent.
Hang onto your stuff sacks or they’ll blow away and create backcountry litter.
Pull on the pole sleeve fabric when inserting poles to avoid any bunching in the material.
Push rather than pull poles through pole sleeves.

Thanks for choosing a Big Agnes tent!
Please feel free to contact us if you have any questions or comments.
support.bigagnes.com | 877.554.8975