BATTLE MOUNTAIN 2 & 3 SET UP INSTRUCTIONS

1. Remove contents from stuff sack Spread out the tent body.

2. Stake out the four corners of the tent body.

3. Assemble the pole set. 2P, assemble one main pole with two 3-way hubs, one pole with two NR joints and one pole with one NR joint. 3P, assemble one main pole with two 3-way hubs, two long pre-bent poles and one short pre-bent pole. To ensure each pole section is fully seated insert each pole section into the next by hand, instead of allowing the shock cord to snap them together.

4. Position the main pole on top of the tent body, aligning it so that the hubs are centered over the body and the ridge pole is running parallel to the doors. Match the colors of the pole ends with the matching colors of the webbing on the tent body and insert the tips of the pole into the grommets. Locate the H clips in the middle of the tent, attach them to the disks on the bottom of the hubs.

5. Attach the corresponding DAC twist clips on the tent body to the main pole.

6. 2P; position the pole with two NR joints over the front door. Match the colors of the pole ends with the matching colors of the webbing on the sides of the tent body and insert the tips of the pole into the grommets. Locate the H clips above the door, attach them to the NR joints. Take the remaining pole, position it over the back door. Match the colors of the pole ends with the matching colors of the webbing on the sides of the tent body and insert the tips of the pole into the grommets on the side of the tent. Locate the H clip above the door, attach it to the NR joint.

7. 3P; position one of the longer pre-bent poles over the front door and one over the rear door. Match the colors of the pole ends with the matching colors of the webbing on the sides of the tent body and insert the tips of the pole into the grommets.

8. Attach the remaining DAC twist clips to the poles. Attach the large hooks over both poles at the four pole intersections.

9. Drape the rainfly over the tent body and match the colors of the webbing on the fly with the webbing on the body.

10. Attach all Velcro tabs on the underside of the fly to the corresponding pole sections for best stability.

11. Make sure the webbing at the corners and sides of the rainfly is completely slackened. Attach the color coded buckles on the fly with the matching color coded buckles on the tent body.

12. 3P; Locate the pole sleeve above the front vestibule door and feed the short pre-bent pole through the sleeve. Insert the pole tips into the second set of grommets at the two front corners of the structure.

13. Tighten the webbing on each buckle as needed to keep the rainfly taut.

14. Stake out the vestibules then stake out all remaining guylines.

Separate 6” length pole segment included for emergency field repair. Slide repair pole over the break to act as a splint.Secure splint in place with tape.

FAST FLY SET UP INSTRUCTIONS

If you purchase the optional Big Agnes footprint for your tent, it will enable you to pitch a Fast Fly shelter while leaving the tent body behind. The Fast Fly configuration requires the footprint, tent fly, poles and stakes.

1. Lay the footprint on the ground and stake out.

2. Assemble the pole set. 2P, assemble one main pole with two 3-way hubs, one pole with two NR joints and one pole with one NR joint. 3P, assemble one main pole with two 3-way hubs, two long pre-bent poles and one short pre-bent pole. To ensure each pole section is fully seated insert each pole section into the next by hand, instead of allowing the shock cord to snap them together.

3. Position the main pole on top of the footprint, aligning it so that the ridge pole is running parallel to the front and back of the footprint. Insert the pole tips into the corner grom-mets.

4. 2P; position the pole with two NR joints over the head end of the main pole. Match the colors of the pole ends with the matching colors of the webbing on the sides of the foot-print and insert the tips of the pole into the grommets. Take the remaining pole, position it over the foot end of the main pole. Match the colors of the pole ends with the match-ing colors of the webbing on the sides of the footprint and insert the tips of the pole into the grommets on the side of the footprint.

5. 3P; position one of the longer pre-bent poles over the head end of the main pole. Match the colors of the pole ends with the matching colors of the webbing on the sides of the footprint and insert the tips of the pole into the grommets. Repeat the step with the second of the longer pre-bent poles over the foot end of the main pole.

6. Drape the rainfly over the pole frame. Match the webbing colors on the fly with the matching colors of the webbing on the footprint.

7. Attach all Velcro tabs on the underside of the fly to the corresponding pole sections for best stability.

8. Make sure the webbing at the corners and sides of the rainfly is completely slackened. Attach the buckles on the fly to those on the footprint.

9. 3P; Locate the pole sleeve above the front vestibule door and feed the short pre-bent pole through the sleeve. Insert the pole tips into the second set of grommets at the two front corners of the footprint.

10. Tighten the webbing on each buckle as needed to keep the rainfly taut.

11. Stake out the vestibules then stake out all remaining guylines.

HELPFUL HINTS FOR TENT SET UP

Our tents are easy to set up but we suggest you practice once at home before using them for the first time to avoid late night bickering with tent mates while fumbling around in the dark.

Before pitching tent, clear campsite of debris that may pierce tent floor.

We recommend staking out all corners, vestibules and guylines to increase space and venti-lation. Securely staking out your tent and all guyline is crucial to maintaining the structural integrity of your tent.

Hang onto your stuff sacks or they’ll blow away and create backcountry litter.

Pull on the pole sleeve fabric when inserting poles to avoid any bunching in the material.

Push rather than pull poles through pole sleeves.

Thanks for choosing a Big Agnes tent!

Please feel free to contact us if you have any questions or comments.

support.bigagnes.com | 877.554.8975